BOLTS

SIZE	LENGTH

(INCH)	WRENCH SIZE	DESCRIPTION/USE	QTY	ORIGINAL P/N	ABINGDON P/N	MOSS P/N

5 - 0.80MM6 - 1MM	5/8	2BA3/16W	CAMSHAFT THRUST PLATECAMSHAFT THRUST PLATE BOLT ACTUALLY FOUND IN 2 ENGINES	2	AAA2356
5 - 84	320-130

5 - 0.75 Mm	1 9/16 1/8 W	FAN TO PULLEY	4	AAA5213	7 - 23	320-120

6 - 1MM	½	3/16W	UPPER REAR MAIN SEAL	3	AAA6142	3 - 12	320-130

6 - 1MM	½	3/16W	ROCKER COVER SIDE BOSSES	3	AAA6142	3 - 12	320-130

6 - 1MM	5/8	3/16W	OIL PICKUP TO BAFFLE	2	JA5117	3 - 169

6 - 1MM	5/8	3/16W	BAFFLE TO SUMP	4	JA5117	3 - 173

6 - 1MM	5/8	3/16W	OIL PICKUP COVER (LATE TD)	1	HP0405	3 - 167

6 - 1MM	1 ½	3/16W	OIL PICKUP TO SUMP, DRILLED FOR SAFETY WIRE	2	ASL5853	3 - 161	320-150

6 - 1MM	1 ½	3/16W	TIMING CHAIN TENSIONER, DRILLED FOR SAFETY WIRE	2	AAA5792	5 - 8	320-150

6 - 1MM	2 5/8	3/16W	OIL PUMP TO BLOCK (EARLY TD)

(LATE TD)	4

2	AAA5586	3 - 99	320-160

6 - 1MM	3 5/16	3/16W	OIL PUMP TO BLOCK, DRILLED FOR SAFETY WIRE (EARLY TD)

(LATE TD)	2	Above and below oil pump bolts in stainless

4	AAA5586	3 - 99	320-160

6 - 1MM	3 ½	3/16W	OIL PUMP TO BLOCK, DRILLED FOR SAFETY WIRE	2	AAA3093	3 - 97	320-170

8 - 1MM	½	3/16W	OIL GALLERY PLUGS	5	X22968	3 - 8	328-100

8 - 1MM	5/8	3/16W	FRONT BEARING PLATE TO BLOCK	2	AAA5343	3 - 40	320-260

8 - 1MM	5/8	3/16W	TIMING CHAIN COVER TO FRONT BEARING PLATE	2	X15012	3 - 39	320-260

8 - 1MM	5/8	3/16W	CAM BEARING DOWEL BOLTS ( DRILLED FOR SAFETY WIRE)	2	AAA5621	5 - 44	320-900

8 - 1MM	3/4	1/4W	CLUTCH TO FLYWHEEL	6	AAA5609	13 - 47	321-028

8 - 1MM	3/4	1/4W	ENGINE MOUNT CRADLE TO FRONT BEARING PLATE	4	ASL5829	3 - 42	320-260

8 - 1MM	3/4	1/4W	GENERATOR ADJUSTING LINK	1	X15012	3 - 149	320-260

8 - 1MM	3/4	1/4W	GENERATOR MOUNTING BRACKET TO BLOCK	2	CA1122	3 - 146	320-260

8 - 1MM	3/4	1/4W	CLUTCH CABLE BRACKET TO SUMP (EARLY TD)	2	CA1122	13 - 31	320-260

8 - 1MM	3/4	1/4W	OIL FILTER SUPPORT BRACKET (EARLY TD)	3	CA1122	USE 3 - 39	320-260

8 - 1MM	3/4	1/4W	TIMING CHAIN COVER TO FRONT BEARER PLATE (2 BOLTS FROM REAR OF BEARER PLATE)	2	CA1122	3 - 39
320-260

8 - 1MM	7/8	1/4W	WATER OUTLET ELBOW TO HEAD (TD)	4	CA1258	3 - 132	320-270

8 - 1MM	7/8	1/4W	AIR CLEANER ELBOW TO CARBURETOR	4	CA1258	3 - 62A	320-270

8 - 1MM	7/8	1/4W	WATER PUMP (SHORT BOLT)	1	CA1258	7 - 27	320-270

8 - 1MM	7/8	3/16W	SUMP TO BLOCK (CENTER BOLTS)	10	LA7431	3 - 74	320-270

8 - 1MM	7/8	3/16W	SUMP TO TIMING CHAIN COVER (DEEP HEAD)	2	AAA5340	3 - 73	320-265

8 - 1MM	1	1/4W	WATER PUMP (LONG BOLT)	1	JA5052	7 - 28	320-625

8 - 1MM	1	*	REAR PLATE TO HEAD (* SCREW HEAD)	4	3 - 50	323-180

8 - 1MM	1	1/4W	BELL HOUSING TO ENGINE	10	JA5052	3 - 58	321-048

8 - 1MM	1	1/4W	BOTTOM GENERATOR MOUNTING	2	X22853	3 - 153/157	320-625

8 - 1MM	1 1/8	3/16W	SUMP TO BLOCK (DEEP HEAD SLOTTED - REAR 2 BOLTS)	2	AAA5341	3 - 75	320-615

8 - 1MM	1 1/4	13MM	GUDGEON PIN CLAMP BOLTS (ORIGINAL BOLTS HAD 1/4W HEADS)	4	CA1009	5 - 17	320-890

8 - 1MM	1 7/8	1/4W	TIMING CHAIN COVER TO ENGINE	3	AAA5286	3 - 36	320-300

8 - 1MM	2	1/4W	TIMING CHAIN COVER TO ENGINE (2 LOWER BOLTS)	2	AAA5231	3 - 35	320-310

8 - 1MM	2 1/4	13MM1/4W	ROD BIG END BOLTS (WITH SELF LOCKING NUTS) (DRILLED FOR COTTER PIN)	8	AEF123	5 - 15	320-880

8 - 1MM	3 5/16	1/4W	ROCKER TOWER	4	AAA5670	5 - 57	320-330

10 - 1.5MM	3/4	5/16W	CARBURETOR TO MANIFOLD	4	320-510

10 - 1.5MM	7/8	3/8W	FLYWHEEL TO CRANKSHAFT, DRILLED FOR SAFETY WIRE	4	AAA5609	13 - 61	321-108

10 - 1.5MM	1	5/16W	STARTER TO BLOCK	2	320-510

10 - 1.5MM	3 ½	5/16W	ROCKER TOWER	4	AAA5692	5 - 58	320-530

12 - 1.5MM	7/8	5/8W	CRANKSHAFT PULLEY BOLT/STARTING DOG (CAN USE 1 1/8 SAE WRENCH)	1	AAA5279	5 - 30	433-450

12 - 1.5MM	1	3/8W19MM	TIMING GEAR TO CAMSHAFT (SOME BOLTS COME WITH THIS LARGER HEAD)	1	AAA5788	5 - 35	320-670

1/4 - 26 BSF	1 1/4	3/16W	ENGINE BREATHER PIPE CLAMP BOLT (SOME OF THESE MAY BE 6 - 1MM)	1	CA1263	USE 23 - 125	320-200

1/4 - 20 W	1 3/8	1/4W	DISTRIBUTOR CLAMP PINCH BOLT (EARLY TD)	1

5/16 -22 BSF	3/4	1/4W	CLUTCH RETURN SPRING BRACKET TO SUMP	1	AJG6255Z	13 - 22	320-360

5/16 -22 BSF	3/4	1/4W	AIR CLEANER TO CARBURETOR (TD MKII)	4	23-185	320-360

5/16 - 18 W	5/8	1/4W	TOP GENERATOR MOUNTING BOLT (5/16 - 18 SAE BOLT FITS)	1	3H2092	3 - 151	322-510

3/8 - 20 BSF	4 ½	5/16W	OIL FILTER HOUSING	1	300852	3 - 197

Studs

SIZE	LENGTH

(INCH)	WRENCHSIZE	DESCRIPTION/USE	QTY	ORIGINAL P/N	ABINGDON P/N	MOSS P/N

6 - 1MM	1 7/8	N/A	TAPPET COVER STUDS	3	AAA5595	3 - 16

8 - 1MM	1 1/4	N/A	WATER OUTLET ELBOW TO THERMOSTAT HOUSING STUD	2	CB1717	3-31	328-730

8 - 1MM	1 7/8	N/A	LONG WATER PUMP STUD	1	X20167	3 - 30	328-750

8 - 1MM	1 3/4	N/A	SHORT WATER PUMP STUD	1	JB5969	3-31	328-750

8 - 1MM	4	N/A	MANIFOLD TO HEAD	4	AAA5773	3 - 47	328-760

8 - 1MM	5 1/4	N/A	ROCKER COVER STUDS	2	AAA5552	3 - 46	328-770

10 - 1.5MM	2	N/A	CARBURETOR TO MANIFOLD STUDS (TD MKII)	4	QA11791	3 - 121	328-810

10 - 1.5MM	1 1/2	N/A	EXHAUST FLANGE TO MANIFOLD STUDS	3	X15126	3 - 62A	328-808

10 - 1.5MM	4 3/8	N/A	HEAD TO BLOCK STUDS	10	AAA5512	3 - 13	328-780

12 - 1.5MM	3 1/8	N/A	MAIN BEARING CAP TO BLOCK STUDS	6	LA7104	5 - 85	328-830

Plugs

SIZE	LENGTH

(INCH)	WRENCH SIZE	DESCRIPTION/USE	QTY	ORIGINAL P/N	ABINGDON P/N	MOSS P/N

10 - 1.5MM	N/A	3/15W	CENTER OIL GALLERY PLUG	1	X20247	3 - 9

12 - 1.5MM	5/16	*	FRONT OIL GALLERY PLUG (*SCREW HEAD, STEEL)	1	X22732	65 - 57	328-020

12 - 1.5MM	9/16	*	REAR OIL GALLERY PLUG (*SCREW HEAD, BRASS)	1	X15393	65 - 57	328-030

12 - 1.5MM	N/A	5/16W	OIL PUMP BODY PLUG (LATE TD)	1	163138	3 - 212

12 - 1.5MM	N/A	5/16W	OIL PUMP COVER	2	10798	3 - 215

12 - 1.5MM	N/A	5/16W	SUMP OIL PICKUP PORT PLUG	1	10798	3 - 215

21 - 1MM	N/A	9/16W	RELIEF VALVE CAP (CAN USE 1" SAE WRENCH)	1	AAA5628	3 - 111

½-14 BSP	N/A	1/2W	SUMP OIL DRAIN PLUG	1	AAA2599	3 - 68	328-120

Nuts

SIZE	LENGTH

(INCH)	WRENCH SIZE	DESCRIPTION/USE	QTY	ORIGINAL P/N	ABINGDON P/N	MOSS P/N

8 - 1MM	N/A	1/4W	WATER PUMP STUD NUT	2	CA1126	3 - 51	311-100

8 - 1MM	N/A	1/4W	WATER OUTLET ELBOW TO THERMOSTAT HOUSING STUD	2	CA1126	USE 3-51	311-100

8 - 1MM	N/A	1/4W	FRONT ENGINE MOUNT CRADLE TO FRONT BEARING PLATE	4	CA1126	3 - 43	311-100

8 - 1MM	N/A	1/4W	MANIFOLD CLAMP NUT	4	CA1126	3 - 66	311-100

8 - 1MM	NA	1/4W13MM	ROD BIG END CAP BOLT NUT (ORIG. CASTELLATED FOR COTTER PIN) ( SELF LOCKING TYPE)	8	AEF131	5 - 16
311-080

10 - 1.5MM	N/A	5/16W	HEAD STUD NUT	10	AAA5208	3 - 56	311-200

10 - 1.5MM	N/A	5/16W	EXHAUST FLANGE TO MANIFOLD NUT (BRASS)	3	CA1605	3 - 63	311-200

12 - 1.5MM	N/A	7/16W	MAIN BEARING CAP STUD NUT (CASTELLATED FOR COTTER PIN)	6	AEF199	5 - 5	311-270

1/4 - 26 BSF	N/A	3/16	ENGINE BREATHER PIPE CLAMP BOLT NUT (SOME OF THESE MAY BE 6 - 1MM)	1	CA1254	USE 23 - 425	311-050

1/4-26 BSF	N/A	3/16W	DISTRIBUTOR COTTER BOLT NUT (LATE TD)	1	CA1254	311-050

1/4 - 20 W	N/A	1/4W	DISTRIBUTOR CLAMP PINCH BOLT NUT (EARLY TD)	1

3/8 - 20 BSF	N/A	5/16W	CLUTCH LINKAGE FULCRUM PIN NUT (CASTELLATED FOR COTTER PIN)	2	AAA5802	13 - 26	311-240

Miscellaneous

SIZE	LENGTH

(INCH)	WRENCH SIZE	DESCRIPTION/USE	QTY	ORIGINAL P/N	ABINGDON P/N	MOSS P/N

2BA	3/4	*	BYPASS ELBOW TO THERMOSTAT HOUSING (*SLOTTED CHEESE HEAD SCREW)	2	AJD320	7-66	323-040

8-1MM	7/8	1/4W	DISTRIBUTOR LOCK BOLT (EARLY TD)	1	AAA5212	35 - 93	433-530

1/4-26 BSF	N/A	N/A	DISTRIBUTOR COTTER BOLT (LATE TD)	1	AAA2776	35 - 90	433-540

3/8-20 BSF	N/A	N/A	CLUTCH LINKAGE FULCRUM PIN	2	X23049	13 - 27	190-390

1/8 BSP	N/A	3/16W	BLOCK WATER DRAIN TAP	1	3H2724	3 - 14	434-240

1/8 BSP	1	5/16W	OIL PIPE BLOCK TO HEAD BANJO BOLT (EARLY TD)

(LATE TD)	2	X21021

AAA5550	3 - 115A

3 - 115	435-465

435-490

1/4 BSP	1 1/8	1/2W	FILTER TO BLOCK OIL PIPE (EARLY TD)	3	X19089	3 - 86	435-480

Torque Values for XPAG Engines

Engine

Description	Torque

GUDGEON PIN CLAMP BOLT	25 LBFT

ROD BIG END BOLTS	25 LBFT

MAIN BEARING CAP NUTS	63 LBFT

FLYWHEEL TO CRANKSHAFT BOLTS	50 LBFT

CLUTCH PRESSURE PLATE BOLTS	19 LBFT

OIL PICKUP PIPE TO SUMP BOLTS	6 LBFT

CAMSHAFT LOCATING PLATE BOLTS	6 LBFT

CAMSHAFT SPROCKET BOLT	50 LBFT

TIMING CHAIN TENSIONER BOLTS	6 LBFT

SUMP TO BLOCK BOLTS	19 LBFT

TIMING CHAIN COVER BOLTS	19 LBFT

CRANKSHAFT PULLEY BOLT	50 LBFT

CYLINDER HEAD NUTS	50 LBFT

ROCKER TOWER BOLTS (8 MM)	16 LBFT

ROCKER TOWER BOLTS (10 MM)	43 LBFT

OIL PUMP TO BLOCK BOLTS	6 LBFT

Other

Description	Torque

WATER PUMP PULLEY NUT	10 LBFT

GENERATOR PULLEY NUT	35 LBFT

TRANSMISSION OUTPUT FLANGE NUT	65 LBFT

REAR AXEL HUB NUT	170 - 200 LBFT

FRONT AXEL HUB NUT	40 - 70 LBFT

WHEEL LUG NUTS	50 LBFT